---------------------------------------------------------------------------------
              Database                                    FIXED LENGTH SECTION
              --------
FSL           'FSL' or 'AWIPS'
---------------------------------------------------------------------------------
              Time Window (use 0,0,0 for default)         FIXED LENGTH SECTION
              -----------
0             Number of minutes relative to nominal time at which to start window
0             Number of minutes relative to nominal time at which to end window
0             0 - return all records within the file containing nominal time
              4 - return all records within *window*
---------------------------------------------------------------------------------
              Providers (see doc/satwnd_providers.txt)    VARIABLE LENGTH SECTION
              ---------
0             0 - default providers (all GOES operational wind products)
              N - list of N provider names follow this line 
---------------------------------------------------------------------------------
              Domain Filter                               FIXED LENGTH SECTION
              -------------
0             0 - don't filter
              1 - return stations within latitude/longitude corners
              2 - return stations within specified Polar Stereographic grid
              3 - return stations within specified Lambert Conformal Conic grid

              Latitude/Longitude Corners (lines skipped if not Domain Filter 1)
              --------------------------
37.0          SW corner latitude (north)   
-109.0        SW corner longitude (east)
41.0          NE corner latitude (north)
-102.0        NE corner longitude (east)

              Polar Stereo Specification (lines skipped if not Domain Filter 2)
              --------------------------
190500.0      Grid box size (meters)
7.838         Latitude (north) of 1st grid point (lower left = SW)
-141.028      Longitude (east) of 1st grid point (lower left = SW)
-95.0         Orientation longitude (east)                 
33.0          I-coordinate of pole
45.0          J-coordinate of pole
60.0          Lat (north) at which X-Y scale is true
65            Number of grid points in X-direction (I dimension)
43            Number of grid points in Y-direction (J dimension)

              Lambert Conformal Conic Specification (lines skipped if not Domain Filter 3)
              -------------------------------------
40635.25      Grid box size (meters)
12.19         Latitude (north) of 1st grid point (lower left = SW)
-133.459      Longitude (east) of 1st grid point (lower left = SW)
-95.0         Orientation longitude (east)
25.0          Latitude (north) of first Lambert Conformal tangent
25.0          Latitude (north) of second Lambert Conformal tangent
185           Number of grid points in X-direction (I dimension)
129           Number of grid points in Y-direction (J dimension)
---------------------------------------------------------------------------------
              QC Filter                                   FIXED LENGTH SECTION    
              ---------
0              0 - none
               1 - coarse
              99 - highest possible
---------------------------------------------------------------------------------
	      Time Selection                              FIXED LENGTH SECTION
              --------------
1             0 - Julian format (YYJJJHHMM)
              1 - Month/Day format (YYYYMMDD_HHMM)
0             0 - Use the nominal time line below
              1 - Use the current time as the nominal time
20090903_1200 Nominal time (in selected format)
---------------------------------------------------------------------------------
              Variables (1 per line, until end of file)   VARIABLE LENGTH SECTION
              --------- (see doc/satwnd_variable_list.txt)
DD        
FF        
U         
V         
HT        
RFF       
QINM      
QIWM      
LSM       
LEVTYPE   
DDIR      
FFIR      
UIR       
VIR       
HTIR      
RFFIR     
QINMIR    
QIWMIR    
LSMIR     
DDVIS     
FFVIS     
UVIS      
VVIS      
HTVIS     
RFFVIS    
QINMVIS   
QIWMVIS   
LSMVIS    
DDWV      
FFWV      
UWV       
VWV       
HTWV      
RFFWV     
QINMWV    
QIWMWV    
LSMWV     
DDS10     
FFS10     
US10      
VS10      
HTS10     
RFFS10    
QINMS10   
QIWMS10   
LSMS10    
DDS11     
FFS11     
US11      
VS11      
HTS11     
RFFS11    
QINMS11   
QIWMS11   
LSMS11    
