---------------------------------------------------------------------------------
              Database                                    FIXED LENGTH SECTION
              --------
FSL           'FSL' or 'AWIPS'
---------------------------------------------------------------------------------
              Time Window (use 0,0,0 for default)         FIXED LENGTH SECTION
              -----------
0             Number of minutes relative to nominal time at which to start window
0             Number of minutes relative to nominal time at which to end window
0             0 - return all records within the file containing nominal time
              1 - return one record per fixed station, closest to nominal time
              2 - return one record per fixed station, closest to start of window
              3 - return one record per fixed station, closest to end of window
              4 - return all records within *window*
---------------------------------------------------------------------------------
              Providers (see doc/map_providers.txt)       VARIABLE LENGTH SECTION
              ---------
0             0 - all providers 
              N - list of N provider names follow this line 
---------------------------------------------------------------------------------
              Domain Filter                               FIXED LENGTH SECTION
              -------------
0             0 - don't filter
              1 - return stations within latitude/longitude corners
              2 - return stations within specified Polar Stereographic grid
              3 - return stations within specified Lambert Conformal Conic grid

              Latitude/Longitude Corners (lines skipped if not Domain Filter 1)
              --------------------------
37.0          SW corner latitude (north)   
-109.0        SW corner longitude (east)
41.0          NE corner latitude (north)
-102.0        NE corner longitude (east)

              Polar Stereo Specification (lines skipped if not Domain Filter 2)
              --------------------------
190500.0      Grid box size (meters)
7.838         Latitude (north) of 1st grid point (lower left = SW)
-141.028      Longitude (east) of 1st grid point (lower left = SW)
-95.0         Orientation longitude (east)                 
33.0          I-coordinate of pole
45.0          J-coordinate of pole
60.0          Lat (north) at which X-Y scale is true
65            Number of grid points in X-direction (I dimension)
43            Number of grid points in Y-direction (J dimension)

              Lambert Conformal Conic Specification (lines skipped if not Domain Filter 3)
              -------------------------------------
40635.25      Grid box size (meters)
12.19         Latitude (north) of 1st grid point (lower left = SW)
-133.459      Longitude (east) of 1st grid point (lower left = SW)
-95.0         Orientation longitude (east)
25.0          Latitude (north) of first Lambert Conformal tangent
25.0          Latitude (north) of second Lambert Conformal tangent
185           Number of grid points in X-direction (I dimension)
129           Number of grid points in Y-direction (J dimension)
---------------------------------------------------------------------------------
              QC Filter                                   FIXED LENGTH SECTION    
              ---------
0              0 - none
               1 - coarse
               2 - screened
              99 - highest possible
---------------------------------------------------------------------------------
	      Time Selection                              FIXED LENGTH SECTION
              --------------
1             0 - Julian format (YYJJJHHMM)
              1 - Month/Day format (YYYYMMDD_HHMM)
0             0 - Use the nominal time line below
              1 - Use the current time as the nominal time
20090903_1200 Nominal time (in selected format)
---------------------------------------------------------------------------------
	      Station Selection                           FIXED LENGTH SECTION
              -----------------
0             0 - Get all stations
              1 - Get only the station whose name is on the next line
SEAWA         Single station name
---------------------------------------------------------------------------------
              Variables (1-4 per line, until end of file) VARIABLE LENGTH SECTION
              --------- (see doc/map_variable_list.txt)
ABA1           
ABA2           
ABA3           
ABA4           
ABA5           
ABE1           
ABE2           
ABE3           
ABE4           
ABE5           
APR1
APW1
APW2
APW3
AVGMIN         
BEAM1          
BEAM2          
BEAM3          
BEAM4          
BEAM5          
CNOB1           
CNOB1W1         
CNOB1W2         
CNOB1W3        
CNOB2           
CNOB2W1         
CNOB2W2         
CNOB2W3        
CNOB3           
CNOB3W1         
CNOB3W2         
CNOB3W3        
CNOB4           
CNOB4W1         
CNOB4W2         
CNOB4W3        
CNOB5           
CNOB5W1         
CNOB5W2         
CNOB5W3        
CPASSR1        
CPASSW1        
CPASSW2        
CPASSW3        
CRECR1         
CRECW1         
CRECW2         
CRECW3         
CSTMR1
CSTMW1
CSTMW2
CSTMW3
CWINR1         
CWINW1         
CWINW2         
CWINW3         
DD               
DDW1            
DDW2            
DDW3            
DG1R1
DG1W1
DG1W2
DG1W3
FF               
FFW1            
FFW2            
FFW3            
GSR1           
GSW1           
GSW2           
GSW3           
HT               
HTR1           
HTW1            
HTW2            
HTW3            
LEVTYPE         
MIXLYR         
NBEAMS         
NCIR1          
NCIW1          
NCIW2          
NCIW3          
NLEVR1
NLEVW1
NLEVW2
NLEVW3
NRMODES        
NSPECR1        
NSPECW1        
NSPECW2        
NSPECW3        
NWMODES        
NYQVR1         
NYQVW1         
NYQVW2         
NYQVW3         
P                
PBLHT
PR1            
PRPR1          
PRPW1          
PRPW2          
PRPW3          
PW1             
PW2             
PW3             
PWR1           
PWW1           
PWW2           
PWW3           
RCNO            
RCNOR1         
RDVB1           
RDVB1W1         
RDVB1W2         
RDVB1W3        
RDVB2           
RDVB2W1         
RDVB2W2         
RDVB2W3        
RDVB3           
RDVB3W1         
RDVB3W2         
RDVB3W3        
RDVB4           
RDVB4W1         
RDVB4W2         
RDVB4W3        
RDVB5           
RDVB5W1         
RDVB5W2         
RDVB5W3        
RSNR            
RSNRR1         
RW              
RWR1           
SNRB1           
SNRB1W1         
SNRB1W2         
SNRB1W3        
SNRB2           
SNRB2W1         
SNRB2W2         
SNRB2W3        
SNRB3           
SNRB3W1         
SNRB3W2         
SNRB3W3        
SNRB4           
SNRB4W1         
SNRB4W2         
SNRB4W3        
SNRB5           
SNRB5W1         
SNRB5W2         
SNRB5W3        
STATYPE        
TV               
TVR1           
TVW              
TVWR1          
U                
UGUST          
USDEV          
UW1             
UW2             
UW3             
V                
VCFLAG1        
VCFLAG2        
VCFLAG3        
VGUST          
VSDEV          
VW1             
VW2             
VW3             
W                
WSDEV          
WW1             
WW2             
WW3             
SNOWLEV
