MADIS Hydro Variables 
-----------------------------------------------------------------------------
Code       Name                                Units      Max       Database
                                                       QC Level*   FSL  AWIPS   
-----------------------------------------------------------------------------
PCP5M     accumulated precip - 5m              m            1       X     X
PCP1H     accumulated precip - 1h              m            1       X     X
PCP3H     accumulated precip - 3h              m            1       X     X
PCP6H     accumulated precip - 6h              m            1       X     X
PCP12H    accumulated precip - 12h             m            1       X     X
PCP24H    accumulated precip - 24h             m            1       X     X
RIVSTG    river stage                          m            0       X     X
RIVFLO    river flow                           (m**3)/s     0       X     X
ELEV      elevation                            m            0       X     X
LAT       latitude                             deg N        0       X     X
LON       longitude                            deg E        0       X     X

MADIS Surface Variables - Character
----------------------------------------------------------------------------------
Code       Name                                Character         Notes  Database
                                               Size                     FSL  AWIPS
----------------------------------------------------------------------------------
STALOC    station location                     51                1       X     X

1. The station location generally contains a geographic description of the 
   station's location, like city and state.

* The QC information is only available with the FSL database.


