ABA1           124   N   antenna beam azimuth   (Beam 1)
ABA2           125   N   antenna beam azimuth   (Beam 2)
ABA3           178   N   antenna beam azimuth   (Beam 3)
ABA4           179   N   antenna beam azimuth   (Beam 4)
ABA5           180   N   antenna beam azimuth   (Beam 5)
ABE1           181   N   antenna beam elevation   (Beam 1)
ABE2           182   N   antenna beam elevation   (Beam 2)
ABE3           183   N   antenna beam elevation   (Beam 3)
ABE4           184   N   antenna beam elevation   (Beam 4)
ABE5           133   N   antenna beam elevation   (Beam 5)
APR1           189   N   RASS averaging period in minutes
APW1           190   N   averaging period in minutes (Mode 1)
APW2           191   N   averaging period in minutes (Mode 2)
APW3           192   N   averaging period in minutes (Mode 3)
AVGMIN         149   N   default averaging period in minutes
BEAM1          134   C   antenna beam name (Beam 1)
BEAM2          135   C   antenna beam name (Beam 2)
BEAM3          136   C   antenna beam name (Beam 3)
BEAM4          137   C   antenna beam name (Beam 4)
BEAM5          138   C   antenna beam name (Beam 5)
CNOB1           13   N   consensus number  (Beam 1)
CNOB1W1         43   N   consensus number  (Beam 1)
CNOB1W2         73   N   consensus number  (Beam 1)
CNOB1W3        103   N   consensus number  (Beam 1)
CNOB2           16   N   consensus number  (Beam 2)
CNOB2W1         46   N   consensus number  (Beam 2)
CNOB2W2         76   N   consensus number  (Beam 2)
CNOB2W3        106   N   consensus number  (Beam 2)
CNOB3           19   N   consensus number  (Beam 3)
CNOB3W1         49   N   consensus number  (Beam 3)
CNOB3W2         79   N   consensus number  (Beam 3)
CNOB3W3        109   N   consensus number  (Beam 3)
CNOB4           22   N   consensus number  (Beam 4)
CNOB4W1         52   N   consensus number  (Beam 4)
CNOB4W2         82   N   consensus number  (Beam 4)
CNOB4W3        112   N   consensus number  (Beam 4)
CNOB5           25   N   consensus number  (Beam 5)
CNOB5W1         55   N   consensus number  (Beam 5)
CNOB5W2         85   N   consensus number  (Beam 5)
CNOB5W3        115   N   consensus number  (Beam 5)
CPASSR1        142   N   minimum no. of RASS records needed to pass consensus
CPASSW1        150   N   mininum number of records needed to pass consensus   
CPASSW2        151   N   mininum number of records needed to pass consensus   
CPASSW3        152   N   mininum number of records needed to pass consensus   
CRECR1         141   N   number of RASS consensus records used
CRECW1         153   N   no. of consensus records used
CRECW2         154   N   no. of consensus records used      
CRECW3         155   N   no. of consensus records used      
CSTMR1         193   C   RASS consensus start time
CSTMW1         194   C   consensus start time (Mode 1)
CSTMW2         195   C   consensus start time (Mode 2)
CSTMW3         196   C   consensus start time (Mode 3)
CWINR1         143   N   RASS consensus window
CWINW1         156   N   consensus window                   
CWINW2         157   N   consensus window                   
CWINW3         158   N   consensus window                   
DD               1   N   wind direction                       
DDW1            31   N   wind direction
DDW2            61   N   wind direction
DDW3            91   N   wind direction
DG1R1          197   N   RASS delay to first gate
DG1W1          198   N   delay to first gate (Mode 1)
DG1W2          199   N   delay to first gate (Mode 2)
DG1W3          200   N   delay to first gate (Mode 3)
FF               2   N   wind speed                       
FFW1            32   N   wind speed
FFW2            62   N   wind speed
FFW3            92   N   wind speed
GSR1           148   N   RASS gate spacing
GSW1           159   N   gate spacing                       
GSW2           160   N   gate spacing                       
GSW3           161   N   gate spacing                       
HT               8   N   geometric height                     
HTR1           128   N   geometric height                   
HTW1            38   N   geometric height
HTW2            68   N   geometric height
HTW3            98   N   geometric height
LEVTYPE         28   N   level type                           
MIXLYR         123   N   mixing layer
NBEAMS         140   N   number of antenna beams used
NCIR1          144   N   RASS number of coherent integrations
NCIW1          162   N   number of coherent integrations    
NCIW2          163   N   number of coherent integrations    
NCIW3          164   N   number of coherent integrations    
NLEVR1         201   N   RASS number of levels
NLEVW1         202   N   number of levels (Mode 1)
NLEVW2         203   N   number of levels (Mode 2)
NLEVW3         204   N   number of levels (Mode 3)
NRMODES        177   N   number of RASS modes used          
NSPECR1        145   N   RASS number of averaged spectra
NSPECW1        165   N   number of averaged spectra         
NSPECW2        166   N   number of averaged spectra         
NSPECW3        167   N   number of averaged spectra         
NWMODES        139   N   number of modes used
NYQVR1         206   N   RASS Nyquist velocity                   
NYQVW1         168   N   Nyquist velocity                   
NYQVW2         169   N   Nyquist velocity                   
NYQVW3         170   N   Nyquist velocity                   
P                9   N   pressure                             
PBLHT          205   N   height of planetary boundary layer
PR1            129   N   pressure                           
PRPR1          147   N   RASS pulse repetition period
PRPW1          171   N   pulse repetition period            
PRPW2          172   N   pulse repetition period            
PRPW3          173   N   pulse repetition period            
PW1             39   N   pressure                             
PW2             69   N   pressure                             
PW3             99   N   pressure                             
PWR1           146   N   RASS pulse width
PWW1           174   N   pulse width                        
PWW2           175   N   pulse width                        
PWW3           176   N   pulse width                        
RCNO            11   N   RASS consensus number                     
RCNOR1         131   N   RASS consensus number
RDVB1           15   N   radial velocity  (Beam 1)
RDVB1W1         45   N   radial velocity  (Beam 1)
RDVB1W2         75   N   radial velocity  (Beam 1)
RDVB1W3        105   N   radial velocity  (Beam 1)
RDVB2           18   N   radial velocity  (Beam 2)
RDVB2W1         48   N   radial velocity  (Beam 2)
RDVB2W2         78   N   radial velocity  (Beam 2)
RDVB2W3        108   N   radial velocity  (Beam 2)
RDVB3           21   N   radial velocity  (Beam 3)
RDVB3W1         51   N   radial velocity  (Beam 3)
RDVB3W2         81   N   radial velocity  (Beam 3)
RDVB3W3        111   N   radial velocity  (Beam 3)
RDVB4           24   N   radial velocity  (Beam 4)
RDVB4W1         54   N   radial velocity  (Beam 4)
RDVB4W2         84   N   radial velocity  (Beam 4)
RDVB4W3        114   N   radial velocity  (Beam 4)
RDVB5           27   N   radial velocity  (Beam 5)
RDVB5W1         57   N   radial velocity  (Beam 5)
RDVB5W2         87   N   radial velocity  (Beam 5)
RDVB5W3        117   N   radial velocity  (Beam 5)
RSNR            12   N   RASS signal-to-noise ratio                     
RSNRR1         132   N   RASS signal-to-noise ratio                     
RW              10   N   RASS w wind component                     
RWR1           130   N   RASS w wind component              
SNOWLEV        207   N   snow level
SNRB1           14   N   signal-to-noise ratio  (Beam 1)
SNRB1W1         44   N   signal-to-noise ratio  (Beam 1)
SNRB1W2         74   N   signal-to-noise ratio  (Beam 1)
SNRB1W3        104   N   signal-to-noise ratio  (Beam 1)
SNRB2           17   N   signal-to-noise ratio  (Beam 2)
SNRB2W1         47   N   signal-to-noise ratio  (Beam 2)
SNRB2W2         77   N   signal-to-noise ratio  (Beam 2)
SNRB2W3        107   N   signal-to-noise ratio  (Beam 2)
SNRB3           20   N   signal-to-noise ratio  (Beam 3)
SNRB3W1         50   N   signal-to-noise ratio  (Beam 3)
SNRB3W2         80   N   signal-to-noise ratio  (Beam 3)
SNRB3W3        110   N   signal-to-noise ratio  (Beam 3)
SNRB4           23   N   signal-to-noise ratio  (Beam 4)
SNRB4W1         53   N   signal-to-noise ratio  (Beam 4)
SNRB4W2         83   N   signal-to-noise ratio  (Beam 4)
SNRB4W3        113   N   signal-to-noise ratio  (Beam 4)
SNRB5           26   N   signal-to-noise ratio  (Beam 5)
SNRB5W1         56   N   signal-to-noise ratio  (Beam 5)
SNRB5W2         86   N   signal-to-noise ratio  (Beam 5)
SNRB5W3        116   N   signal-to-noise ratio  (Beam 5)
STATYPE        188   N   station type
TV               6   N   virtual temperature                     
TVR1           126   N   virtual temperature                
TVW              7   N   virtual temperature with vertical wind correction
TVWR1          127   N   TV corrected for vertical wind     
U                3   N   u wind component                     
UGUST          118   N   u wind component gust
USDEV          120   N   u wind component std dev             
UW1             33   N   u wind component                     
UW2             63   N   u wind component                     
UW3             93   N   u wind component                     
V                4   N   v wind component                     
VCFLAG1        185   N   vertical correction flag (Mode 1)
VCFLAG2        186   N   vertical correction flag (Mode 2)
VCFLAG3        187   N   vertical correction flag (Mode 3)
VGUST          119   N   v wind component gust
VSDEV          121   N   v wind component std dev             
VW1             34   N   v wind component                     
VW2             64   N   v wind component                     
VW3             94   N   v wind component                     
W                5   N   w wind component                     
WSDEV          122   N   w wind component std dev             
WW1             35   N   w wind component                     
WW2             65   N   w wind component                     
WW3             95   N   w wind component                     
